Configuration of the FROG on a Cisco ISR router

Before starting this guide you should check to have all the devices needed:


* Cisco ISR router with a IOS version 15.2M or greater
* An additional UCS integrated blade server and a 4 or 8 ports EHWIC
* One or more standard Intel servers for the remote controller

During the testing phase we used a Cisco ISR 2911 (IOS 15.3) with a UCS E140S as hardware and Ubuntu 14.04 LTS with KVM as hypervisor (both for the controller and the UCS).

# Environment analysis

This system has been designed and tested having a precise scenario in mind, but it is flexible and can be adapted for many different cases, in order to fit the constraints of different environment. This guide will try to provide proper suggestions for every possible case.

The scenario the system has been designed for is the following:



The orchestrator is not connected through a dedicated management network (as suggested instead in the Openstack installation guide) because it is supposed to be remote; it could be somewhere on the corporate geographic network or even on the Internet! But if you don’t need this feature, you can choose to have a local orchestrator connected with a separate management network, consequently increasing traffic separation and security.

On the other hand, we strongly recommend not installing the orchestrator on the UCS server, because the resulting CPU load could be too much for this kind of machines. In fact, the orchestrator is composed of three different services (Openstack controller, Opendaylight and a custom orchestrator) which should be installed into separated virtual machines. This configuration prevents having three different physical servers with a low CPU and RAM load, but it is still possible to deploy these services on separated servers or wherever you like.


# Router configuration

The basic steps for setting the ISR (with a UCS-E blade) up can be found at the following page:

<http://www.cisco.com/c/en/us/td/docs/unified_computing/ucs/e/1-0/gs/guide/b_Getting_Started_Guide/b_Getting_Started_Guide_preface_00.html>

Particularly, the interesting part of the above manual is from the beginning till the “Accessing CIMC” section.

At this point, we are assuming that the basic configuration of the device is already completed. When the devices are properly working, you can start deploying the architecture shown below:



The picture shows how we designed the system and how the traffic should flow through the router, the server and the network functions chains installed on it. Basically, all the traffic exchanged between the enterprise LAN and the Internet is forced to pass through the chains.

The interfaces named “*ucse*” are internal and provide access to the UCS server with a high speed connection. The *slot*/0 one simulates a L3 interface, while the *slot*/1 one simulates a L2 interface. The other ends of these links can be seen on the server side as *eth0* and *eth1*.


## Virtual functions connection

The link that connects the server with the router, through the L3 ucse1/0 interface, can be configured in many ways, depending on the configuration choices you made in the previous step (e.g., the presence of a dedicated management network) and on the availability of public IP addresses in your network.

* If it is possible, you can assign a public subnet on the link that brings from interface *ucse1/0* to *eth0* (more precisely to a virtual switch called br-ex). The dimension of that subnet should be larger enough to support the maximum number of chains created on the UCS server and also an additional address for the management network endpoint, if you don’t have a separate one on another interface. That’s a large pool!
* In case you decide to use a NAT (as in our test case) you can instead aggregate all chains addresses on a single dynamic “overloaded” translation (that means you are using a PAT) but you must use a static translation for the management address, if not separated. This configuration could be useful for security and address saving.

In both cases, you should consider having a DHCP instance for the *ucse1/0* interface.

Since the first case is easier to configure, we present now an example configuration with NAT:

*ip dhcp excluded-address 192.168.0.1*

*ip dhcp excluded-address 192.168.0.2*

*ip dhcp pool dhcp-pool*

*import all*

*network 192.168.0.0 255.255.255.0*

*default-router 192.168.0.1*

*dns-server 8.8.8.8*

*interface ucse1/0*

*ip address 192.168.0.1 255.255.255.0*

*ip nat inside*

*interface GigabitEthernet0/1*

*ip address 130.192.225.244 255.255.255.128*

*ip nat outside*

*ip nat pool natpool 130.192.225.242 130.192.225.242 prefix-length 25*

*ip nat inside source list 7 pool natpool overload*

*ip nat inside source static 192.168.0.2 130.192.225.243*

*ip route 0.0.0.0 0.0.0.0 GigabitEthernet0/1 130.192.225.254*

*access-list 7 deny 192.168.0.2*

*access-list 7 permit 192.168.0.0 0.0.0.255*

## Users connection

The link that connects users through the EHWIC module is simpler to configure. The only thing needed is an address-less VLAN for letting lv2 traffic, like ARP and DHCP, pass and Opendaylight check users MAC addresses for users separation.

*interface ucse1/1*

*switchport access vlan 2*

*no ip address*

*interface Vlan2*

*no ip address*

*no spanning-tree vlan 2*

*interface GigabitEthernet0/0/n*

*switchport access vlan 2*


*no ip address*

## Logical configuration of the network in the UCS blade

In order to better understand the configuration of the router, we present here the internal virtual topology that will be built soon, while installing the software components on the UCS server. This is what was identified by the box “virtual functions chains” in previous image on page 3. Please note that this entire configuration is created automatically by Openstack and our custom orchestrator; you don’t have to create manually any of these switches.

The role of each virtual switch is pretty simple, but it is extremely important to deeply understand that in case you need some troubleshooting.

* Br-ex is the exit point of all the virtual machines traffic and, in our configuration, also of the controller management traffic
* Br-int is where Openstack places all its virtual machines. Due to our customization, the last link is no more with br-int but directly with br-ex, so we have as many links as the number of functions graphs between br-int and br-ex (everyone with its own IP public address)
* Br-usr is where the user network is (directly or not) connected with a layer 2 link



The only thing you should configure is the addresses on br-ex switch, eth0 and eth1 interfaces, using the */etc/network/interfaces* configuration file (in Ubuntu). Follows an example of that configuration, where the addresses used are the same of the example configuration with NAT explained in the previous page. Please adapt it to your real environment.

*auto br-ex*

*iface br-ex inet static*

*address 192.168.0.2*

*netmask 255.255.255.0*

*gateway 192.168.0.1*

*dns-nameservers 8.8.8.8 4.4.4.4*

*auto eth0*

*iface eth0 inet manual*

*auto eth1*

*iface eth1 inet manual*

Of course also eth2 can be configured for some special purpose, for example:

* As Openstack tunnel interface, for connections with other compute nodes
* As Opestack dedicated management interface with a local controller
* As an emergency port for management access to the server


## Server “emergency port”

Since wrong configuration of virtual switches or Opendaylight flows could lead to packet loops and (as mentioned later) Opendaylight sometimes take over the control of all virtual switches, it would be extremely important to configure the management port of the UCS server or, as an alternative, the external *eth2* interface for management access. That port is completely separated from the entire internal virtual infrastructure, so it is guaranteed to be immune from loops.

In case you want to use the *eth2* interface, you can configure a static address on it and, when connecting a laptop, use an address of the same subnet. Otherwise you can configure on that interface a dhcp daemon for Ubuntu (<https://help.ubuntu.com/community/isc-dhcp-server>).


# Software installation

The system is the result of a deep integration and customization of different software and open-source “off-the-shelf” products. For this reason, it could be hard to understand well its structure and behaviors at first sight.



The figure above illustrates the different software components that belong to the two main nodes. The blue ones are three logical sub-modules of the cloud orchestrator Openstack, while the red ones are SDN controller and the global orchestrator. The virtualized network layers allow virtual machines interconnection and consist of the group of virtual switches already presented in the previous paragraph (the one on the controller is simpler as it is only one switch).

## Controller virtual machine setup

On the controller node you need one virtual switch to connect the three controller virtual machines to the outside world using a public IP address. Of course this is not true anymore if you decided to separate them on different servers.

You can create your bridge by yourself, using Openvswitch or Linux Bridge and Virt-manager. Then, you should give a public IP address to the switch, exactly as explained previously.

Through virt-manager (requires GUI), you should set the bridge you created as the default NIC for every VMs:

* Launch *virt-manager*
* Right click on the machine you’re configuring, and select “open”
* In the new window, select “View->Details”
  + Select “Specify shared device name” as source device
  + Type the name of the bridge you want to connect in the “bridge” box
  + Select “virtio” as device model

Now you have to modify also the XML description of the virtual machine, by typing:

“*virsh edit "vm name"*

In the *<interface type ='bridge'>* tag add these lines (immediately after *<source ..>* tag):

*<virtualport type = 'openvswitch'>*

*<parameters interfaceid = 'ext-net-uuid'/>*

*</virtualport>*

You can simply type the global UUID of the Openvswitch switch. Although this is not formally correct, as the UUID should belong to the Openvswitch bridge, currently it works. In case you want to generate a new UUID and assign it to the bridge, possibly modifying also the */etc/network/interfaces* file, you can follow those steps:

[*http://www.itechlounge.net/2014/03/linux-how-to-generate-uuid-for-network-interface-on-rhelcentos/*](http://www.itechlounge.net/2014/03/linux-how-to-generate-uuid-for-network-interface-on-rhelcentos/)


In alternative, if you used Linux Bridge to create the switch you have not to do this trick and it works more smoothly, without modifying the XML description, as explained here:

[*http://www.dedoimedo.com/computers/kvm-bridged.html*](http://www.dedoimedo.com/computers/kvm-bridged.html)

## Openstack

The biggest module of the system is a deeply modified version of Openstack. For this reason, you must install the Icehouse stable version. During the development phase we leveraged the official guide (<http://docs.openstack.org/icehouse/install-guide/install/apt/content/>) for the installation and the configuration of components of interest.

When reading the proposed guide you will probably find a bit confusing the part about networking and interfaces configuration (the Openstack networking module used is neutron).

It supposes to have three different physical nodes but our system is designed with the compute and the network node both on the UCS server, so they use the same interfaces. You can instead choose where to place the controller and how to configure the management network. With a separated management network you need at least an additional interface on the UCS (you can use eth2 for this role); otherwise the management and “external” interfaces will be unite on the same physical interface (eth0). The tunnels endpoint interfaces are for connection between network node and compute nodes, or between many compute nodes. Since we have the two nodes on the same physical server and only one compute node, you can forget about these interfaces.

The software components of interest for our system are only the following ones:

* Basic environment
* Identity service (Keystone)
* Image service (Glance)
* Compute service (Nova)
* Networking service (Neutron)
* Orchestration service (Heat)
* Dashboard (Horizon)
* Command line clients for each one of them

We suggest also installing Phpmyadmin on the controller, to get database operations easier.

**Note**: when following the guide pay attention to use file hosts shortcuts only when the guide does it, because some service (like VNC in *nova.conf*) need to have IP addresses explicitly indicated.

**Note**: if you run into a problem when installing some **clients** (e.g., **keystone**) such as “error: command 'x86\_64-linux-gnu-gcc' failed with exit status 1”, please install the following packages:

*# Install python-dev  
sudo apt-get install python-dev*

*#Upgrade to the newest version of ‘pip’ (the one in the Ubuntu 14.04 repository is too old, it will generate an error when installing netifaces; see* [*http://stackoverflow.com/questions/27341064/how-do-i-fix-importerror-cannot-import-name-incompleteread*](http://stackoverflow.com/questions/27341064/how-do-i-fix-importerror-cannot-import-name-incompleteread) *)  
easy\_install -U pip*

*# Install the ‘netifaces’ module  
sudo pip install netifaces*

**Note**: if you run into a problem when installing some **clients** (e.g., **glance**) such as “c/\_cffi\_backend.c:13:17: fatal error: ffi.h: No such file or directory”, please install the following packages:

*sudo apt-get install libffi-dev libssl-dev*

**Then, you have to force the reinstall of the failed package:**

*pip install --upgrade --force-reinstall [package\_name, e.g., python-glanceclient]*

**Note**: if you run into some problems when installing **nova-api** service and the log shows you a problem like "*No module named rootwrap.cmd*" or something similar, you can try to copy */usr/lib/python2.7/dist-packages/oslo/rootwrap/* in */usr/local/lib/python2.7/dist-packages/oslo* and then restart. Alternatively, you can install that package with “pip”.

## Openstack extension

All the Openstack code modifications are done on the controller node. To get easier this phase and not to get people too confused we created a repository with all the code organized in folders which represent the various Openstack components and, in each one, we created a bash script called “install\_extension” which is in charge to do almost everything. Please install our modifications following the order shown below and not in alphabetical order.

The virtual machines images are present in a separate git repository.

* Neutron: simply launch the script with sudo privileges:
  + *sudo ./Neutron-extension/install\_extension.sh*
* Neutron-client: simply launch the script with sudo privileges:
  + *sudo ./Neutron-client-extension/install\_extension.sh*
* Heat:
  + Open the configuration file */etc/heat/heat.conf* and set the value “*plugin\_dirs*” to the directory */usr/lib/heat-extensions*
  + Launch the script: *sudo ./Heat-extension/install\_extension.sh*
* Keystone: use the usual script:
  + *sudo ./Keystone-extension/install\_extension.sh*
* Glance:
  + Load the virtual machines onto Glance repository (with Horizon or command line)
  + Create a new “m1.little” flavor in the admin panel with 1 CPU, 2048MB RAM, 40GB hard disk, no ephemeral disk (0GB) and no swap partition (0GB). This is the flavor that best fit our VMs and maximize performances.
* Horizon (optional):
  + These plugins are optional and can help users build their NFV graphs
  + Forwarding graph extension is thought for letting admin manage graphs created by all users directly from the Horizon admin panel and can be installed with the script: *sudo ./Horizon-extension/Forwarding\_graph/install\_extension.sh*
  + Service graph extension is the opposite panel in the Horizon project panel and allows each user to design his own graph with a simple “drag and drop” gui. The script is: *sudo ./Horizon-extension/Service\_Graph/install\_extension.sh*
* CreateProfile web page (optional):
  + This web page is useful for the admin to directly manipulate graphs descriptions into the orchestrator database (as an alternative of Horizon extension).
  + Install some needed software: *sudo apt-get install curl libcurl3 libcurl3-dev php5-curl*
  + Insert the page on apache: s*udo cp –r CreateProfile/ /var/www/html/*
  + Restart apache: *sudo service apache2 restart*

## Opendaylight

If you install Opendaylight on a virtual machine, you should assign it at least 2 cores and 2GB of RAM memory, because it is a complex software.

Again, you should follow the official Opendaylight controller installation guide provided by their website (<https://wiki.opendaylight.org/view/OVSDB:OVSDB_OpenStack_Guide>). You must be sure to configure ODL in order to use OpenFlow 1.0 and not the 1.3 version (commands are in the above guide).

We also recommend setting a value of “MaxPermSize” equal or greater than 2048m.

Once the installation is completed, you should stop the service named SimpleForwarding using Opendaylight OSGI interface or, even better, remove the file

"*org.opendaylight.controller.samples.simpleforwarding\*.jar*"

from "*plugins*" directory (that will prevent it from automatically run at startup).

**IMPORTANT**: before giving ODL the control of your infrastructure you must prevent it from controlling the exit point toward the outside world of your network node; otherwise you won't even be able to reach it if it is remote!! You can do it with a cron script that deletes controller from br-ex external virtual bridge (more details following).

**Note**: OpenDaylight does not often start in the proper way. In order to check that it is running correctly, (i) wait at least 1 minute (more is even better) in order to allow this software to initialize, (ii) type the command “lb” (“list bundles”), which shows the current status of all the OSGI bundles. If the software is ok, most of the bundles (some isolated exceptions are in fact present) are marked as “Active”.

If everythying is ok, you should be able to access to the web interface, connecting to the IP address of the ODL controller on port 8080:

<http://myopendaylightIP:8080> [admin/admin]

## Integrating ODL into the OpenStack infrastructure

First, you should avoid OpenStack to keep the control of the br-ex switch. For this, it is better

On the **compute** node, create a cron script like the one below (for the root user):

*\* \* \* \* \* ovs-vsctl del-controller br-ex*

Now we can set Opendaylight as the preferred ml2 plugin for Openstack. On the **controller** node, we have to modify the Neutron configuration file */etc/neutron/plugins/ml2/ml2\_conf.ini* as follows. If some fields or some sections are missing add them (sections can be placed at the end of the file).

*[ml2]*

*…*

*mechanism\_drivers = opendaylight*

*….*

*[ovs]*

*local\_ip = controller*

*tunnel\_type = gre*

*enable\_tunneling = True*

*tenant\_network\_type = gre*

*tunnel\_bridge = br-tun*

*int\_peer\_patch\_port = patch-tun*

*[odl]*

*network\_vlan\_ranges = 1:4095*

*tunnel\_id\_ranges = 1:1000*

*tun\_peer\_patch\_port = patch-int*

*int\_peer\_patch\_port = patch-tun*

*tenant\_network\_type = gre*

*tunnel\_bridge = br-tun*

*integration\_bridge = br-int*

*[ml2\_odl]*

*# (StrOpt) OpenDaylight REST URL*

*# If this is not set then no HTTP requests will be made.*

*#*

*url = http://opendaylight:8080/controller/nb/v2/neutron*

*# Example: url = http://192.168.56.1:8080/controller/nb/v2/neutron*

*# (StrOpt) Username for HTTP basic authentication to ODL.*

*#*

*username = admin*

*# Example: username = admin*

*# (StrOpt) Password for HTTP basic authentication to ODL.*

*#*

*password = admin*

*# Example: password = admin*

*# (IntOpt) Timeout in seconds to wait for ODL HTTP request completion.*

*# This is an optional parameter, default value is 10 seconds.*

*#*

*timeout = 10*

*# (IntOpt) Timeout in minutes to wait for a Tomcat session timeout.*

*# This is an optional parameter, default value is 30 minutes.*

*#*

*session\_timeout = 30*

Finally, on the **compute** node, you can set Opendaylight as the manager for the Openswitch infrastructure:

*ovs-vsctl set-manager tcp:xxx.xxx.xxx.xxx:6640*

(where xxx.xxx.xxx.xxx indicates the public ip address of Opendaylight controller)

At the end, stop and remove from startup list the service "*neutron-plugin-openvswitch-agent*" on all the **compute** nodes because it can create some conflicts with Opendaylight normal operations.

This can be achieved by creating a file “*/etc/init/neutron-plugin-openvswitch-agent.override*” and writing the keyword “*manual*” in it.

## Custom orchestrator

First of all copy the folder named "*Orchestrator*" into your virtual machine (or server).

Then install all the necessary software:

*sudo apt-get install python-dev python-setuptools*

*sudo easy\_install pip*

*sudo apt-get install python-sqlalchemy libmysqlclient-dev*

*sudo pip install --upgrade cython falcon requests gunicorn jsonschema mysql-python json\_hyper\_schema*

Some tables must be added on the **controller** node mysql database:

*mysql -u root -p*

*CREATE DATABASE orchestrator;*

*GRANT ALL ON orchestrator.\* TO 'orchestrator'@'%' IDENTIFIED BY 'orchestrator\_db\_password';*

*GRANT ALL ON orchestrator.\* TO 'orchestrator'@'localhost' IDENTIFIED BY 'orchestrator\_db\_password';*

*USE orchestrator;*

*CREATE TABLE session (id VARCHAR(64) NOT NULL PRIMARY KEY, user\_id VARCHAR(64), mac\_address Text, session\_info Text, profile Text, infrastructure Text, started DATETIME, last\_update DATETIME, error DATETIME, ended DATETIME);*

*CREATE TABLE profile (id VARCHAR(64) NOT NULL PRIMARY KEY, profile Text);*

*CREATE TABLE component\_adapter (session\_id VARCHAR(64) NOT NULL PRIMARY KEY, extra mediumtext NOT NULL);*

*CREATE TABLE endpoint (Graph\_ID VARCHAR(64) NOT NULL, Endpoint\_ID VARCHAR(64) NOT NULL, Available tinyint(1) NOT NULL, Name VARCHAR(64) NOT NULL, ID VARCHAR(64) NOT NULL, Type VARCHAR(64) DEFAULT NULL, Graph\_ID\_connected VARCHAR(64) DEFAULT NULL, Endpoint\_ID\_connected VARCHAR(64) DEFAULT NULL, PRIMARY KEY (Graph\_ID,Endpoint\_ID));*

*exit*

In order to adapt the system to the current machine, you should change some configuration into the **orchestrator virtual machine**. You can find it in *Orchestrator/Configuration/orchestrator.conf*.

*[orchestrator]*

*port = 8000*

*# isp and nobody are particular working modes*

*isp = false*

*nobody = false*

*debug\_mode = false*

*[authentication]*

*# controller openstack*

*server = http://x.x.x.x:35357*

*orch\_username = admin\_username*

*orch\_password = admin\_password*

*orch\_tenant = admin*

*admin\_tenant\_name = admin*

*admin\_user = admin\_username*

*admin\_password = admin\_password*

*[user\_connection]*

*# ingress port where br-int receives traffic from users*

*ingress\_type = physical*

*ingress\_port = INGRESS\_to-br-usr*

*#egress physical port where the traffic will exit (port bridged to br-ex)*

*egress\_type = physical*

*egress\_port = eth0*

*[db]*

*# controller openstack*

*connection = mysql://orchestrator:orchestrator\_db\_password@x.x.x.x/orchestrator*

*[ovs\_agent]*

*#openstack network node address (br-ex)*

*endpoint = http://y.y.y.y:11223*

*#virtual switch where virtual machines are connected*

*switch\_to\_connect = br-int*

*#virtual switch where all the users traffic will go out*

*exit\_switch = br-ex*

Change the image id into the "Templates" directory with the IDs assigned from Openstack to the virtual machines images loaded onto Glance

Set the address of the controller into the orchestrator machine file hosts

Now you should insert Opendaylight and orchestrator IP addresses in controller and compute nodes hosts file, because some configuration files use this references for getting addresses.

## Custom orchestrator agent

The last step to complete is to install the orchestrator agent on the network node. First of all, copy the folder “Orchestrator-agent” on that node and install the same python component you installed on the controller node. Then you can install and run it thanks to pre-configured scripts:

*cd Orchestrator-agent/*

*sudo ./install\_agent.sh*

*sudo ./start.sh*

Note that, from now on, it will start at boot time without any further operation.

We can finally run the orchestrator by typing:

*cd UNorchestrator/Orchestrator*

*./start\_orchestrator.sh*

## Troubleshooting Opendaylight

In our experience, rather often ODL fails to control the network in the proper way.

In this case we suggest the following procedure in order to restart all the network components:

* [**OS controller**]: Delete all the stacks that are active (with our external tools; not from the OpenStack console)
* [**OS controller**]: Delete all remaining instances of networks, routers, VMs
* [**OS controller**]: Stop the neutron server (*# service stop neutron-server*)
* [**ODL**]: Quit ODL (just CTRL+C in the ODL console)
* [**OS compute**]: Delete the controller and management connection from the virtual switch to ODL (you can launch the *del\_manager.sh* script in the “Useful-scripts” folder)
* [**ODL**]: Start ODL and make sure that most of the OSGI bundles are marked as “active”
* [**OS compute**]: Re-assign the manager to OVS (use the script *set\_manager.sh* script in the “Useful-scripts” folder)
* [**OS compute**]: Make sure that ODL took control of the switches, and that all the switches have only a flow to the controller and another called “NORMAL” (this can be done by issuing the command *#ovs-ofctl dump-flows [bridgename]*)
* [**OS controller**]: Restart neutron server on the controller

# Creation and instantiation of network functions

Actually, there are many ways to instantiate NFVs chains; every one follows some specific needs. For example with the “nobody” system, one service graph is created at the first setup and then every user who attaches a device to the network will be redirected to a captive portal where he will be forced to login before having the possibility to use it.

Other services are mostly for demonstration and they can be created by hand with some dedicated scripts like:

*cd Orchestrator*

*python instantiate\_cisco\_demo1.py* or *python instantiate\_cisco\_demo2.py*

Since every graph is intended to be used from a precise user, these instantiation scripts need to be configured with the credentials of their user (simply open them and change the parameters user, tenant and password in the first lines of the python file).

At the moment of writing, these graphs need also to be deleted by another script. We recommend not to delete the stack from Horizon gui because it does not clean our custom data structures!

*cd Orchestrator*

*python delete\_cisco\_demo1.py* or *python deletecisco\_demo2l.py*

If you decide to use the graphs with user recognition capabilities (i.e. isp and nobody), you should take care of Openstack default quotas. Since these graphs use a lot of networks and subnets, you must enlarge quotas of isp and nobody tenants:

source Useful-scripts/admin-openrc.sh

neutron quota-update --tenant\_id xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx --network 50

neutron quota-update --tenant\_id xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx --subnet 50

You can also modify default quotas permanently in the /etc/neutron/neutron.conf configuration file.

There is also a simple web page that does nothing but calling these scripts when the user presses the correspondent button on the web GUI. If you want to try it, you can find it in “*Useful-tools*” directory and install it exactly like CreateProfile.